|  |  |  |
| --- | --- | --- |
| **Annex to the contract pursuant to DE-UZ 53**  **Environmental Label for**  **"Construction Machinery"** |  | **Please use this**  **printed form!** |

Applicant (label holder):

The applicant is a  Manufacturer

Importer

Operator

The application is a  Type-based application

Single application

Brand/trade name:

Type of construction machine[[1]](#footnote-1):

Type no. for the construction machine (see Table 1):

(corresponds to Annex I of Directive 2000/14/EC)

Combustion process:

(petrol engine/diesel engine)

Net installed power or       kW

electrical output1:

Guaranteed sound power level LWAd:       dB (A)

(see 3.1.1.)

Sound pressure level LpA (see 3.1.2):       dB (A)

Emission of air pollutants

Output:       kW

CO:       g/kWh

Particle mass:       g/kWh

Particle number:       Particles per kWh

NOx:       g/kWh

HC:       g/kWh

Declaration by the manufacturer / importer

It is hereby declared that

* the construction machine is correspondingly marked in accordance with Article 11 of Directive 2000/14/EC. The EC Declaration of Conformity is available and enclosed. Information on the section of the machine where the guaranteed sound power level is indicated and, where relevant, the section of the product documentation where this value can be found has been provided.
* a declaration guaranteeing the durability of the technology used for reducing emissions for 5 years is enclosed.
* In the case of type-based applications, a technical service provider shall be commissioned to carry out annual CoP inspections of the proper functionality of the exhaust gas handling system based on the Swiss Guidelines for at least 5 construction machines of each type and the reports shall be submitted to RAL gGmBH on request as verification.
* Information is provided in the operating instructions that it is not permitted to make any changes to the construction machine that will lead to an increase in the noise emissions or the exhaust emissions.

Declaration by the operator

It is hereby declared that

* the construction machine is correspondingly marked in accordance with Article 11 of Directive 2000/14/EC. Information on the section of the machine where the guaranteed sound power level is indicated and, where relevant, the section of the product documentation where this value can be found has been provided.
* In the case of single applications, a technical service provider shall be commissioned to carry out an annual inspection of the proper functionality of the exhaust gas handling system based on the Swiss Guidelines and this report shall be submitted to RAL gGmBH on request as verification.
* no changes will be made to the construction machine that lead to an increase in the noise emissions or the exhaust emissions.

Annexes

* Test report in accordance with Paragraph 3.1.2
* EC Declaration of Conformity (for manufacturers/importers)
* Information on the section of the machine where the guaranteed sound power level is indicated and, where relevant, the section of the product documentation where this value can be found.
* Test report in accordance with Paragraph 3.2.1
* Declaration guaranteeing the durability of the technology used for reducing emissions   
  (for manufacturers/importers)

Location:       Applicant:

(legally binding signature

Date:       and company stamp)

1. 1 An annex must be completed for every different type and performance class of construction machine. [↑](#footnote-ref-1)