|  |  |  |
| --- | --- | --- |
| **Annex 2b to the Contract pursuant to DE-UZ 65**  **Blue Angel Eco-Label for**  **„Unbleached Filter Papers for Use with Hot and Boiling Water“** |  | **Please use this**  **form !** |

Pulp Manufacturer

(full address):

Emission values:

**during pulp manufacture expressed as annual averages**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Lower Reference Value according to BREF** | **Actual Value** |
| Wastewater volume flow  (process water without cooling water) | 35 m3/ADT \* | m3/ADT \* |
| COD (Chemical Oxygen Demand) | 8 kg/ADT | kg/ADT |
| BOD5 (Five-day Biochemical Oxygen Demand) | 1.5 kg/ADT or 25 mg/l | kg/ADT |
| Filterable substances | 1.4 kg/ADT | kg/ADT |
| AOX | < 0.01 kg/ADT | kg/ADT |
| Total N (inorganic + organic N) (TNb) | 0.2 kg/ADT or 15 mg/l | kg/ADT |
| Total P | 0.02 kg/ADT or 1 mg/l | kg/ADT |

\* ADT = **A**ir **d**ried **t**on

Authorized signature and company stamp

of the pulp manufacturer .................