|  |  |  |
| --- | --- | --- |
| **Annex 2a to the Contract pursuant to DE-UZ 65**  **Blue Angel Eco-Label for**  **„Unbleached Filter Papers for Use with Hot and Boiling Water“** |  | **Please use this**  **form !** |

Manufacturer of the filter paper        
(Direct discharger, Indirect discharger,

Manufacturer of tea filters)

(full address):

-Direct discharger (all limits are complied with)

-Indirect discharger (wastewater volume flow / AOX) are complied with;   
additional parameters are specified)

-Manufacturer of tea filters (the parameters are specified)

Emission values:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Target Value** | **Actual Value**\* |
| Wastewater volume flow | 10 m3/ADT [[1]](#footnote-1)\* |  |
| COD (Chemical Oxygen Demand) | 0.4 kg/ADT |  |
| BOD5 (5-day Biochemical Oxygen Demand) | 0.15 kg/ADT or 25 mg/l |  |
| Filterable substances | 0.2 kg/ADT |  |
| AOX | < 0.01 kg/ADT |  |
| Total N (inorganic + organic N) (TNb) | 0.05 kg/ADT or 15 mg/l |  |
| Total P | 0.003 kg/ADT or 1 mg/l |  |

\* ADT = **A**ir **d**ried **t**on

Authorized signature and company stamp

of the manufacturer of filter papers .................

1. [↑](#footnote-ref-1)