|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Checklist** | |  |
|  |  |  |  |
|  | **DE-UZ 76 – Edition January 2026** | Construction and Furnishing Panels for Interior Construction |  |
|  |  |  |  |

**Checklist DE-UZ 76**

Overview:

1. Verifications that must be provided by ALL applicants
2. Verifications to be submitted depending on product composition/properties
3. Recurring verifications after application approval (every 2 years)

**a) To be provided by ALL applicants:**

|  |  |
| --- | --- |
|  | **Annex 1** Applicant's declarations regarding the contract (form) |

**3.1 General substance requirements**

|  |  |
| --- | --- |
|  | **Overview** of the **structure/composition** of the products(form - **Annex 2**) |
|  | Verification of compliance with the **building regulations requirements** through **technical data** **sheets** and **building authority usability certificates** |
|  | **Safety data sheets** and **technical data sheets** for binders and coatings used (stains, primers, clear coats, topcoats, films, decorative papers, adhesives, etc.) |
|  | **Manufacturer's declaration** of compliance with material requirements(form **– Annex 4**) |

**3.2 Manufacturing process**

**3.2.1 Source of wood and paper**

|  |  |
| --- | --- |
|  | **Annual record of (recycled) wood, cork, bamboo and (recycled) paper content - relating to the product to be certified** (form - **Annex 2**) |
|  | **CoC-certificate** for the production site OR submission of **confirmation** from an **approved auditor** confirming the requirement |
|  | **Sample delivery notes**, with corresponding certification statement |

**3.2.2 Energy statement**

|  |  |
| --- | --- |
|  | **Energy statement** of the production plant (with a focus on renewable energy in accordance with EU guideline 2018/2001/EU) |

**3.2.3 Environmental product declaration (in accordance with DIN EN 15804)**

|  |  |
| --- | --- |
|  | Submission of the **EPD reference** (form – **Annex 1**) |
|  | OR: Confirmation of receipt of the EPD order |

**3.4 Use**

|  |  |
| --- | --- |
|  | **Emission test report** in accordance with DIN EN 16516 and VDI 4301 Sheet 7 (accredited testing institute, not older than two years at the time of application) |
|  | **Test report on odour testing** in accordance with DIN ISO 16000-28 in conjunction with VDI 4302 |

**3.4.5 Product information and consumer information**

|  |  |
| --- | --- |
|  | **Consumer information, technical data sheet, product label** |

**3.5.1 Take-back scheme (optional)**

|  |  |
| --- | --- |
|  | Enclose **confirmation of participation** in the relevant scheme  and  **Consumer information** |

**3.6 Advertising claims**

|  |  |
| --- | --- |
|  | **Technical data sheet** |

**b) The following verifications must be submitted depending on the product composition/ properties:**

**3.1 General substance requirements**

|  |  |
| --- | --- |
|  | If unknown: **Proof of SVHC content** (< 0.1% (w/w)) in accordance with **DIN 51012:2025-03** Overview analyses (screenings) for substances of very high concern |

**3.2.5** **Special requirements for expanded glass granulate panels**

|  |  |
| --- | --- |
|  | Submission of a test report (not older than two years) on non-detectable bisphenol A (extraction method, HPLC-MS). |

**3.3.3 Melamine**

|  |  |
| --- | --- |
|  | **Test report** for detection of melamine in wood-based materials according to **DIN EN 18079:2024-05** |

**3.3.5 Pollutant requirements for recyclability**

|  |  |
| --- | --- |
|  | Test report in accordance with **Annex IV of the Waste Wood Regulation** (AltholzV) in compliance with the specified limit values.  **Not** to be provided for **solid wood products**. |

**3.4.2 Additional emissions test for expanded glass granulate panels**

|  |  |
| --- | --- |
|  | **Test reports** from a recognized testing laboratory must be submitted.  A sample taken from the middle of a stack of expanded glass granulate panels must not emit bisphenol A at 60 °C in a µ chamber. The **detection limit** is **0.5 µg/m³.** |

**c) Recurring verifications after application approval:**

**every 2 years:**

**3.2.1 Source of wood and paper**

|  |  |
| --- | --- |
|  | **Annual record of (recycled) wood, cork, bamboo and (recycled) paper content - relating to the product to be certified** (form - **Annex 2**) |
|  | **CoC-certificate** for the production site OR submission of **confirmation** from an **approved auditor** confirming the requirement |
|  | **Sample delivery notes**, with corresponding certification statement |

**3.2.2 Energy statement**

|  |  |
| --- | --- |
|  | **Energy statement** of the production plant (with a focus on renewable energy in accordance with EU guideline 2018/2001/EU) |

**3.3.5 Pollutant requirements for recyclability**

|  |  |
| --- | --- |
|  | Test report in accordance with **Annex IV of the Waste Wood Regulation** (AltholzV) in compliance with the specified limit values.  **Not** to be provided for **solid wood products**. |

**3.4 Use**

|  |  |
| --- | --- |
|  | **Emission test report** in accordance with DIN EN 16516 and VDI 4301 Sheet 7 (accredited testing institute, not older than two years at the time of application) |
|  | **Test report on odour testing** in accordance with DIN ISO 16000-28 in conjunction with VDI 4302  **(required if the product is advertised as low odour!)** |