|  |  |  |
| --- | --- | --- |
| **Annex to the Contract pursuant to DE-UZ 32**  **Environmental Label for "Water-saving Flushing Boxes"** |  | **Please use**  **this form!** |

Manufacturer (Applicant):

Distributor (Label User):

Brand / Trade Name:

Flushing box (model designation)[[1]](#footnote-1):

Test certificate:

* valid until:

Maximum flushing-water volume:

Adjustable flushing-water quantity for

uninterrupted flushings:

Designation of the devices for a reduction of the

flushing-water volume[[2]](#footnote-2):

The flushing box is equipped with a device for the

interruption of the flushing according to DIN 19542,

para. 3.2.4.2).

The partial flushing-water volume amounts to:

**Declaration of the Applicant**

It is hereby stated that:

* the material identification data according to DIN 54840 are indicated on the flushing box and its components,
* the flushing box is adjusted ex works to a water quantity of 6 litres.
* the flushing box does not exceed the value of the fitting-noise-level Lap for the characteristic flow or flow pressure of 20 dB (A), measured pursuant to DIN 52218, Parts 1 and 2.

**Annex**

* Product information (e.g. informative brochures)
* Test certificate of the Institut für Bautechnik/general certificate of construction supervising authority2
* Description according to 4.3

|  |  |  |  |
| --- | --- | --- | --- |
| **Place:** |  |  |  |
|  |  |  |
| **Date:** |  |  |

**Legally binding signature /company stamp**

1. One "Annex to the Contract" shall be completed for each different flushing-box model. [↑](#footnote-ref-1)
2. Please delete what does not apply. [↑](#footnote-ref-2)