|  |  |  |
| --- | --- | --- |
| **Annex 1 to the Contract pursuant to DE-UZ 99**  **Environmental Label for**  **"Movement Area De-icers for Airfields"** |  | **Please use**  **this printed form!** |

Manufacturer (applicant):

Distributor (label user):

Brand/trade name:

* The applicant declares that the following substances have not been added:
* Triazoles as anti-corrosion protection
* Perfluorinated and polyfluorinated chemicals (PCs)
* Alkylphenol ethoxylate (Octylethoxylate or Nonylethoxylate)
* The complexing agents EDTA and NTA
* The following heavy metals are only contained to a maximum level of 0.1 mg/kg in the product:
* arsenic (As), cadmium (Cd), chromium (Cr), copper (Cu), lead (Pb), mercury (Hg), nickel (Ni).
* The de-icer corresponds to the applicable requirements for its fitness for purpose and safety.
* The de-icing effect has been experimentally proven in a standard process.
* The technical requirements for the products in accordance with SAE, AMS 1435 for liquid de-icer or AMS 1431 for solid de-icer are observed.
* The relevant reports are enclosed.

Location:       Applicant:

Date:       (Legally binding signature

and company stamp)