|  |  |  |
| --- | --- | --- |
| **Annex 1 to the Contract pursuant to DE-UZ 119**  **Environmental Label for**  **„Mattresses“** |  | **Please use this**  **form!** |

Manufacturer (Applicant):

*(full address)*

Brand/Trade name:

**Textiles**

Available covers (diverse materials)

(trade name)

**Product Materials:**

* Fraction of wood + wood-based materials       percent by volume

**Declaration**

**3.1 General substance requirements**

We hereby declare that the materials (leather, textiles, upholstery materials, coating materials[[1]](#footnote-1), adhesives1, etc.) used for the product are not permitted to contain any substances with the following properties as a constituent component:

1. Substances which are identified as particularly alarming under the European Chemicals Regulation REACH (1907/2006/EC) and which have been incorporated into the list drawn up in accordance with Article 59, Paragraph 1 of the REACH Regulation (so-called "list of candidates").[[2]](#footnote-2)

2. Substances that according to the CLP Regulation[[3]](#footnote-3) have been classified in the following hazard categories or which meet the criteria for such classification.

* Carcinogenic in categories Carc. 1A or Carc. 1B
* Germ cell mutagenic in categories Muta. 1A or Muta. 1B
* Reprotoxic (teratogenic) in categories Repr. 1A or Repr. 1B
* Acute toxicity (poisonous) in categories Acute Tox. 1 or Acute Tox.2
* Specific target organ toxicity in categories STOT SE 1, STOT SE 2, STOT RE 1 or STOT RE 2

The corresponding H phrases for the hazard classes and categories can be found in Supplement A.

3. Substances that are classified in TRGS 905[[4]](#footnote-4) as:

* Carcinogenic (K1, K2)
* Mutagenic (M1, M2)
* Reprotoxic (RF1, RF2)
* Teratogenic (RF1, RF2)
  + - 1. Origin oft he wood

The applicant is certified themselves according to FSC or PEFC criteria for the chain of custody (CoC). The certificate is attached here to. Additionally, a record, which specifies the percentage of the used certified woods is attached here to (Annex 2 to the contract DE-UZ 38)

***or***

The applicant submits appropriate certificates from its raw material suppliers. Additionally, a record, which specifies the percentage of the used certified woods is attached here to (Annex 2 to the contract DE-UZ 38)

***or***

The applicant submit other appropriate verifications according to Appendix A of DE-UZ 38 (Annex 3 to the contract DE-UZ 38

No wood is used

* + 1. Formaldehyde in Wood-Based Materials

Only the wood-based material entitled to use the Environmental Label according to DE-UZ 76 is used for the product. (Annex 2)

***or***

Attached is a test report according to the test method for

wood-based materials (Federal Health Bulletin 10/91 p. 488-489)

A test report in accordance to DE-UZ 76 is attached

***or***

Attached is a test certificate confirming the classification into emission class E1

* + 1. Textiles

- Declaration from the textile manufacturer in accordance with the requirements 3.2.2.1 to 3.2.2.5 pursuant to Annex 3 is attached

- No textiles are used

- No coated textiles are used

* + 1. Upholstery Materials

Please Note: Compliance verification will only be required if the respective portion of upholstery materials exceeds 5 percent by volume of the total volume of the piece of upholstered furniture.

- No upholstery materials are used

-Annex 4 is attached

* + - 1. Wires and Springs

- The applicant declare that a closed cleaning/degreasing system is used to degrease and/or clean the wires and/or springs with organic solvents

- The applicant declare that the springs are not covered with a

galvanic metallic layer

* + 1. Indoor air quality

- Test report in accordance with the BAM test method is attached

- Test report is not required

* + 1. Odour

- Test report in accordance with DIN ISO 16000-28 in combination with VDI 4302

*Alternatively:*

-Test report in accordance with RAL-GZ430

* + 1. Fitness for use

- The mattresses must meet the standard quality requirements for fitness for use taking into account the following standards: DIN EN 1334, DIN EN 1725 and DIN EN 1957

- Cot mattresses shall additionally meet the requirements of DIN EN 16890

- Test report according to DIN EN 16890 is attached

- Test report pursuant to EN 1957 about the loss in height and the loss in strength is attached

-Test certificate of the pre-supplier about the ash content of the original material in accordance with DIN 3451-1/2008 is attached

* + 1. Removable mattress cover

- A description and picture of the washing instruction is attached

- Test report according to ISO 6330 in connection with EN 25077 is attached

* 1. Recycling and disposal

- With a view to recycling and disposal neither material protection agents (fungicides, insecticides, flame retardants) nor halogenated organic compounds (e.g. chloroorganic carriers in textiles) may be added to mattresses, including the materials used for the manufacture (textiles, foams, wood-based materials, adhesives etc.).

Exempted from this requirement are biocides exclusively used for in-can preservation in aqueous adhesives as well as adhesives based on aqueous dispersions.

- Declarations form the pre-suppliers are attached

* 1. Consumer information

The Consumer Information providing at least the following basic

information is attached

• Manufacturer / distributor (including address)

• Model name

• Product description, including information on material structure

• Hardness value

• Suitability for adjustable spring bases

• Information on the overall durability (loss in height and strength)

• Information on the product's wear resistance (fields of application and, if applicable, results of material tests, product-specific properties, changes resulting from product use)

• Cleaning and care instructions

• If available, information on take-back

* 1. Advertising claims

Advertising messages must not include any notes such as „tested for its biological living quality" or those which would play down risks in terms of Article 25, para. 4 of Regulation (EC) No 1272/2008 (CLP Regulation), as, for example "nontoxic", "nonharmful". Product designations containing the term "organic" or "bio" shall not be permissible. The same applies to designations like "health mattresses", "mattresses for persons suffering from intervertebral disc problems", "mattresses for allergic persons" and the like.

Place:       Applicant:

Date:       (authorized signature and company stamp)

1. The used materials in the product has to comply the requirements in 3.1.2 general substance requirements for coating systems pursuant to DE-UZ 38 [↑](#footnote-ref-1)
2. The version of the list of candidates at the time of the declaration is valid. The list of candidates in its relevant version can be found at: <http://echa.europa.eu/chem_data/authorisation_process/candidate_list_table_en.asp>. [↑](#footnote-ref-2)
3. Regulation(EG) No. 1272/2008 on classification, labelling and packaging of substances and mixtures, short: CLP Regulation (Classification, Labelling and Packing). It replaces the old directives 67/548/EEC (Dangerous Substances Directive) and 1999/45/EC (Dangerous Preparations Directive). [↑](#footnote-ref-3)
4. TRGS 905, directory of carcinogenic, mutagenic or teratogenic substances from the Committee for Hazardous Substances (AGS): [TRGS 905.](http://www.baua.de/de/Themen-von-A-Z/Gefahrstoffe/TRGS/TRGS-905.html) The current version at the time of application is valid. The CMR complete list published by the Institute for Occupational Safety and Health of the German Social Accident Insurance can also be used as a reference tool (amalgamation of the CMR substances according to the CLP Regulation and TRGS 905): [CMR complete list](http://www.baua.de/de/Themen-von-A-Z/Gefahrstoffe/Einstufung-und-Kennzeichnung/CMR-Gesamtliste_content.html). [↑](#footnote-ref-4)