|  |  |  |
| --- | --- | --- |
| **Annex 5 to the Contract pursuant to DE-UZ 175**  **Blue Angel Eco-Label for „Hair Dryer“** |  | **Please use this  form!** |

**Manufacturer or Supplier Declaration**

**on Plastic Materials**

For application for Use of the Blue Angel Eco-Label

for **Hair Dryers** according to DE-UZ 175

by (name of the company):

based in:

we hereby confirm compliance with the

requirement for the plastic (trade name):

Please provide detailed information.

|  | **Yes** | **No** |
| --- | --- | --- |
| The plastic used for housings and housing parts is free from flame retardants  (except for: plastic parts less than 25 grams in mass). |  |  |
| If “NO”, the plastic contains the following flame retardants:  - Product name:  - Content in weight percent:  - Chemical specification (CAS No.): |  |  |
| The maximum level of fluoroorganic additives in the plastic used for housings and housing parts does not exceed 0.5% by weight. |  |  |
| Except for process-related, technically unavoidable impurities as well as except for plastic parts less than 25 grams in mass, the plastic used for housings and housing parts is |  |  |
| * free from halogenated polymers and additions of organic halogenated compounds used as flame retardants (with the exception of fluoroorganic additives) |  |  |
| * free from flame retardants which are marked with Risk Phrase R 50/53 or Hazard Phrase H 410 according to Part 3 of Annex VI to Regulation (EC) No 1272/2008. |  |  |
| Except for process-related technically unavoidable impurities and except for fluoroorganic additives as constituent components no substances have been added to the plastic used for housings and housing parts (≥ 25 g in mass) which are classified, as: |  |  |
| 1. carcinogenic in categories 1 or 2 according to Table 3.2 or in categories 1A and 1B according to Table 3.1 of Annex VI to Regulation (EC) No 1272/2008[[1]](#footnote-1) 2. mutagenic in categories 1 or 2 according to Table 3.2 or in categories 1A and 1B according to Table 3.1 of Annex VI to Regulation (EC) No 1272/2008 3. reprotoxic in categories 1 or 2 according to Table 3.2 or in categories 1A and 1B according to Table 3.1 of Annex VI to Regulation (EC) No 1272/2008 4. persistent, bioaccumulative and toxic (PBT substances) or very persistent and very bioaccumulative (vPvB substances) according to the criteria of Annex XIII to the REACH Regulation or particularly alarming for other reasons and included into the List (so-called list of candidates[[2]](#footnote-2)) set up in accordance with the REACH Regulation, Article 59, paragraph 1. |  |  |

Confirmed by the company

(Plastic Manufacturer/Supplier):

|  |  |  |  |
| --- | --- | --- | --- |
| **Place:** |  |  |  |
|  |  |  |
| **Date:** |  |  |

**Legally binding signature /company stamp**

1. Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on classification, labelling and packaging of substances and mixtures, amending and repealing Directives 67/548/EEC and 1999/45/EC, and amending regulation (EC) No 1907/2006 [↑](#footnote-ref-1)
2. Link to the list of candidates of Regulation (EC) No. 1907/2006 concerning the Registration, Evaluation, Authorization, and Restriction of Chemicals (REACH):   
   <http://echa.europa.eu/consultations/authorisation/svhc/svhc_cons_en.asp> [↑](#footnote-ref-2)