|  |  |  |
| --- | --- | --- |
| **Annex 1 to the contract pursuant to DE-UZ 188**  **Environmental label for “Vacuum Cleaners”** |  | **Please use this printed form!** |

Manufacturer (Applicant):

Distributor (Label User):

Brand/trade name:

Type designation:

| **Paragraph** | **Declarations/compliance verifications for vacuum cleaners** | **Yes** | **No** |
| --- | --- | --- | --- |
| **3.1** | **Rated input power** |  |  |
|  | The rated input power of the appliance during active operation is ≤ 800 watts. |  |  |
|  | The rated input power during active operation on carpet is       watts. |  |  |
|  | The rated input power during active operation on hard floor is       watts. |  |  |
|  | A test report on the rated input power measured in accordance with EN 60335-1, EN 60335-2-2 or EN 60335-2-69. | **Annex 2** |  |
|  | The rated input power is specified in the product information. **Page** | **Annex 3** |  |
| **3.2** | **Annual energy consumption** |  |  |
|  | The appliance has an annual energy consumption of ≤ 28 kWh/a. |  |  |
|  | The corresponding product information in accordance with Regulation (EC) No. 666/2013 or for cordless vacuum cleaners in accordance with the prEN (IEC) 62885-4 is enclosed with the application. **Page** | **Annex 3** |  |
| **3.3** | **Dust pick up on carpet and hard floor** |  |  |
|  | The appliance has a dust pick up on carpet of > 0.85 (85%). |  |  |
|  | The appliance has a dust pick up on hard floor of > 1.07 (107%). |  |  |
|  | The corresponding product information in accordance with Regulation (EC) No. 666/2013 or for cordless vacuum cleaners in accordance with the prEN (IEC) 62885-4 is enclosed with the application. **Page** | **Annex 3** |  |
| **3.4** | **Dust re-emissions** |  |  |
|  | The household vacuum cleaner has a dust re-emission rate of ≤ 0.01%. |  |  |
| **or** | The commercial vacuum cleaner has a dust re-emission rate of ≤ 0.01%. |  |  |
| **or** | The cordless floor vacuum cleaner has a dust re-emission rate of ≤ 0.1%. |  |  |
|  | The corresponding product information in accordance with Regulation (EC) No. 666/2013 or for cordless vacuum cleaners in accordance with the prEN (IEC) 62885-4 is enclosed with the application. **Page** | **Annex 3** |  |
| **3.5** | **Noise emissions and motion resistance** |  |  |
|  | The noise emissions on carpet are ≤ 73dBA (re 1 pW). |  |  |
| **or** | For appliances with an electric, mechanical or airflow-driven active nozzle:  The noise emissions on carpet are ≤ 78dBA (re 1 pW). |  |  |
|  | The noise emissions on carpet are       dBA. |  |  |
|  | A test report on the noise emissions measured in accordance with DIN EN 60704-1 or DIN EN 60704-3 and DIN EN 60704-2-1 or DIN EN 60335-2-69 is enclosed. | **Annex 4** |  |
|  | The motion resistance with the universal floor nozzle on the test carpet is ≤ 40 N. |  |  |
|  | The motion resistance with the universal floor nozzle on the test carpet is       N. |  |  |
|  | A test report on the motion resistance measured in accordance with EN 60312-1:2017 is enclosed. | **Annex 5** |  |
|  | The noise emissions and motion resistance are specified in the product information in accordance with Regulation (EC) No. 666/2013 or for cordless vacuum cleaners in accordance with the prEN (IEC) 62885-4. **Page** | **Annex 3** |  |
| **3.6** | **Material requirements for plastics used in the housing, housing parts and accessory parts (suction tube/hose, nozzle, etc.)** |  |  |
|  | The applicant declares compliance with all of the requirements according to Paragraph 3.6 of the Basic Award Criteria. |  |  |
|  | The manufacturer's declaration about the plastic materials is enclosed with the application. | **Annex P-M** |  |
|  | A list of which plastics are used in the housing for parts with a mass ≥ 25 grams is enclosed with the application. | **Annex P-L25** |  |
| **3.7** | **Easy-to-maintain and recyclable design and PCR plastic**  The applicant declares compliance with all of the requirements according to Paragraph 3.7 of the Basic Award Criteria. |  |  |
|  | Instructions for dismantling the appliance for those handling old appliances is enclosed. | **Annex 6** |  |
| **3.8** | **Durability requirements** |  |  |
| **3.8.1** | **Durability of household vacuum cleaners**  The applicant declares compliance with all of the requirements according to Paragraph 3.8.1 of the Basic Award Criteria. |  |  |
| **or** | A test report on the durability of the appliance in accordance with DIN EN 60312-1 and a test report on the service life of the motor in accordance with DIN EN 60312-1:2017 are enclosed. | **Annex 7** |  |
| **3.8.2** | **Durability of cordless vacuum cleaners**  The applicant declares compliance with all of the requirements according to Paragraph 3.8.2 of the Basic Award Criteria. |  |  |
|  | An in-house test report on the durability of the appliance is enclosed. | **Annex 7** |  |
| **3.8.3** | **Provision of spare parts** |  |  |
|  | The applicant guarantees the provision of spare parts for at least 8 years following the termination of production. |  |  |
|  | The applicant undertakes to offer a technical aftersales service and to provide this service, as well as technical repairers and consumers of these spare parts, with access to technical documents and, if relevant, repair documentation. |  |  |
|  | Information on the availability of spare parts is included in the product information.  **Page** | **Annex 3** |  |
| **3.9** | **Consumer information** |  |  |
|  | The product documentation includes information on the annual energy consumption for cordless and mains-operated vacuum cleaners and the average rated input power (watts) in operation for mains-operated vacuum cleaners (displayed in table form where possible). **Page** | **Annex 3** |  |
|  | The product documentation includes information on the dust pick up and dust re-emissions. **Page** | **Annex 3** |  |
|  | The product documentation includes information on the noise emissions. **Page** | **Annex 3** |  |
|  | The product documentation includes information on the type of battery, battery life and battery charging cycle, as well as information on the maintenance, replaceability and disposal of the battery. | **Annex 3** |  |
|  | The product documentation includes information on how to replace the dust bag or empty the dust box and filter, as well as information on how to clean the nozzle. **Page** | **Annex 3** |  |
|  | The product documentation includes information on the weight (kg), the proportion of recycled PCR material (%), the operating range (m) for mains-operated vacuum cleaners and the availability of spare parts and where to source them. **Page** | **Annex 3** |  |
|  | The product documentation includes information and instructions on using the vacuum cleaner on carpet and hard floor by means of clear and adjustable settings on the appliance.  **Page** | **Annex 3** |  |

**Annexes to the contract**

Please use this printed form of Annex 1 to the contract.

Please enclose Annexes 2 to 6, Annex P-M and Annex P-L25 with the application documentation:

|  |  |
| --- | --- |
| Annex 2: | A test report on the rated input power measured in accordance with EN 60335-1, EN 60335-2-2 or EN 60335-2-69 |
| Annex 3: | Product information in accordance with Regulation (EC) No. 666/2013 or for cordless vacuum cleaners in accordance with the prEN (IEC) 62885-4 |
| Annex 4: | A test report on the noise emissions measured in accordance with DIN EN 60704-1 or DIN EN 60704-3 and DIN EN 60704-2-1 or DIN EN 60335-2-69 |
| Annex 5: | A test report on the motion resistance measured in accordance with EN 60312-1:2017 |
| Annex 6: | Instructions for dismantling the appliance for those handling old appliances |
| Annex 7: | A test report on the durability of the appliance in accordance with DIN EN 60312-1 and a test report on the service life of the motor in accordance with DIN EN 60312-1:2017  An in-house test report on the durability of the appliance for cordless vacuum cleaners |
| Annex P-M: | Manufacturer/distributor declaration on the plastics materials  (printed form) |
| Annex P-L25: | Manufacturer/distributor declaration on the plastics materials > 25 g (printed form) |

Location:

Date:

Applicant:

(Legally binding signature

and company stamp)