|  |  |
| --- | --- |
| **Annex 4 to the contract**  **according to DE-UZ 217a  THIS ANNEX IS FOR: Applicants as direct dischargers** | **Please only use this form!** |

Environmental label for “Paper made from 100% recovered paper

for paper bags and boxes“

Table 3-2 Maximum limits for the average annual emission parameters (waste water) in the paper production process (not valid for the production of special papers)

Please tick the box if appropriate and complete the table:

**PAPER FACTORY WITH DEINKING:**

|  |  |  |
| --- | --- | --- |
| Parameter | Maximum limit for waste water emissions  (average annual value as a load or concentration) | Measured ACTUAL VALUE (please also state the units) |
| Volumetric flow rate of waste water | <15 m3/Adt |  |
| COD | < 3 kg/Adt |  |
| BSB5 | < 0.15 kg/Adt or <25 mg/l |  |
| AOX | < 0.01 kg/Adt |  |
| Total N (inorganic + organic N) (TNb) | 0.07 kg/Adt or 15 mg/l |  |
| Total P | 0.008 kg/Adt or 1.2 mg/l |  |

Please tick the box if appropriate and complete the table:

**PAPER FACTORY WITHOUT DEINKING:**

|  |  |  |
| --- | --- | --- |
| Parameter | Maximum limit for waste water emissions  (average annual value as a load or concentration) | Measured ACTUAL VALUE (please also state the units) |
| Volumetric flow rate of waste water | <5 m3/Adt |  |
| COD | < 1.2 kg/Adt |  |
| BSB5 | < 0.15 kg/Adt or <25 mg/l |  |
| AOX | < 0.01 kg/Adt |  |
| Total N (inorganic + organic N) (TNb) | 0.07 kg/Adt or 15 mg/l |  |
| Total P | 0.008 kg/Adt or 1.2 mg/l |  |

\* Adt = **A**ir **d**ried **t**on

|  |  |  |  |
| --- | --- | --- | --- |
| **Location:** |  |  |  |
|  |  |  |
| **Date:** |  |  |

**Legally binding signature / company stamp  
of the applicant**