|  |  |
| --- | --- |
| **Annex 1 to the contract pursuant to DE-UZ 206**  **Environmental label for "Garden tools"** | **Please use this printed form!** |

Distributor (Label holder):

Manufacturer:

Brand/trade name:

Type designation[[1]](#footnote-1):

Type of tool:

Nominal consumption (W):

Blade speed (rpm):

Declared sound pressure level LWAd (see 3.1.1):            dB(A)

Cutting width (only for lawnmowers):

Type of drive (mains power, rechargeable battery):

**Declaration by the applicant** (Please delete as appropriate)

|  |  |  |
| --- | --- | --- |
| **Paragraph** | **Declarations/Compliance Verifications** | **Please complete the appropriate sections!** |
| **1.4** | **Compliance with legal requirements** |  |
|  | The applicant declares compliance with existing laws and ordinances. These include e.g.:   * The 32nd Ordinance for the implementation of the Federal Immission Protection Act (BImSchV) * The German Product Safety Act * The German Battery Act * Regulation (EC) 2023/1230 * Regulation (EC) 2023/1542 * Regulation (EC) No. 1103/2010 * EU Directive 2006/66/ECorm * The German Electrical and Electronic Equipment Act * The German Material Ordinance for Electrical and Electronic Equipment * Substance requirements according to Regulation (EC) 1907/2006 and Regulation (EC) No. 1272/2008 * Occupational safety regulation on noise and vibration (LärmVibrationsArbSchVEinfV) |  |
| **3.1** | **Noise emissions** |  |
|  | The applicant declares compliance with the requirements according to Paragraph 3.1 and Table 1. |  |
|  | A test report to verify the A-weighted sound power level *LW*A is enclosed. | **Annex 2** |
|  | Verification of the labelling of the stated sound power level (e.g. a photo) is enclosed. | **Annex 3** |
| **3.2** | **Requirements for batteries (rechargeable batteries)** |  |
| **3.2.1.1** | **Standardisation and interoperability** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.2.1.1. |  |
|  | The relevant pages of the product documentation or a link to the manufacturer’s website are enclosed. |  |
|  | **Pages** | **Annex 13** |
| **3.2.1.2** | **Reduced scope of delivery** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.2.1.2. |  |
|  | Places where the tool can be purchased without accessories: |  |
| **3.2.1.3** | **Removability** |  |
|  | It is possible for the user to remove or separate the rechargeable battery from the tool without damaging it. |  |
|  | The relevant pages of the product documentation are enclosed.  **Pages** | **Annex 13** |
| **3.2.2** | **Testing the capacity of the rechargeable battery (rated capacity)** |  |
|  | The tested battery capacity of three rechargeable batteries is at least 100% of the rated capacity stated by the manufacturer in accordance with EN 61960.  The tested battery capacity is **Ah** |  |
|  | A test report on the capacity of the rechargeable battery is enclosed. | **Annex 5** |
| **3.2.3** | **Low level of self-discharge (charge retention)** |  |
|  | Three rechargeable batteries still display at least 90% of the stated charge retention in tests according to Paragraph 3.2.3.  The tested self-discharge is  **%** |  |
|  | A test report on the self-discharge of the rechargeable battery is enclosed. | **Annex 6** |
| **3.2.4** | **Durability of the rechargeable batteries** |  |
|  | **Warranty cover** |  |
|  | The manufacturer provides a 24 month warranty from the date of purchase on the rechargeable batteries for hobby tools and a 36 month warranty from the date of purchase on the rechargeable batteries for professional tools. |  |
|  | After 24 or 36 months, the residual capacity of the rechargeable battery is at least 70% of the rated capacity. |  |
|  | The relevant pages of the product documentation are enclosed.  **Pages** | **Annex 13** |
|  | **Alternative to a warranty** |  |
|  | The test report for the endurance test of the rechargeable battery is enclosed. |  |
|  |  | **Annex 4** |
|  | The relevant pages of the product documentation are enclosed. |  |
|  | **Pages** | **Annex 13** |
| **3.2.5** | **Replacement rechargeable batteries** |  |
|  | Subsequent purchase of the rechargeable batteries is still possible at least 5 years after the termination of production. Information to this effect is contained in the product documentation. |  |
|  | **Pages** | **Annex 13** |
| **3.2.6** | **Heavy metal content** |  |
|  | The heavy metal content of the rechargeable batteries does not exceed the values stated in Table 2. |  |
|  | A test report carried out using at least 4 rechargeable batteries to test the heavy metal content of the rechargeable batteries is enclosed. | **Annex 7** |
| **3.2.7** | **Guaranteeing the take back of old batteries** |  |
|  | The applicant declares that they comply with the statutory registration and take back obligations of the manufacturer of the batteries.  Registration number (Batt-Reg. No. DE) of the battery manufacturer: |  |
| **3.2.8** | **General safety requirements for the rechargeable battery system** |  |
|  | The applicant declares compliance with the applicable test requirements in accordance with EN/IEC 62133 for the relevant rechargeable battery system. |  |
|  | A test report on the general safety requirements of the rechargeable battery is enclosed. | **Annex 8** |
| **3.2.9** | **No load power consumption of the charging device** |  |
|  | The no load power consumption of the charging device is a maximum of 1.0 watts. |  |
|  | A test report on the no load power consumption of the charging device is enclosed. | **Annex 9** |
| **3.2.10** | **Protection against over-discharging and deep discharging of the rechargeable battery** |  |
|  | The rechargeable battery is protected against over-discharging and deep discharging. |  |
|  | A test report on the protection against over-discharging and deep discharging is enclosed. | **Annex 10** |
| **3.2.11** | **Charging status indicator** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.2.11. |  |
|  | The relevant pages of the product documentation are enclosed.  **Pages** | **Annex 13** |
| **3.3** | **Other requirements for all tools** |  |
| **3.3.1** | **Take back of old tools** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.3.1. |  |
|  | The relevant pages of the product documentation are enclosed. |  |
|  | **Pages** | **Annex 13** |
| **3.3.2** | **Recyclable design of the products** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.3.2. |  |
|  | The relevant pages of the product documentation are enclosed.  **Pages** | **Annex 13** |
| **3.3.3** | **Repairability** |  |
|  | The applicant declares compliance with the requirements in Paragraph 3.3.3. |  |
|  | The relevant pages of the product documentation are enclosed. |  |
|  | **Pages** | **Annex 13** |
| **3.3.4** | **Exclusion of harmful substances in the tools** |  |
|  | The applicant declares compliance with EU Directive 2011/65/EU. The tool does not contain any substances listed in Annex II and III of the directive. |  |
|  | A declaration of conformity with the ROHS Directive is enclosed. | **Annex 11** |
| **3.3.5** | **Material requirements for plastics used in the housing and housing parts** |  |
|  | The applicant declares compliance with the requirements for plastics according to Paragraph 3.3.3. |  |
|  | The corresponding declarations from the plastics manufacturer are enclosed (please use preprinted forms). | **Annex P-M**    **Annex P-L** |
| **3.3.6** | **Additional exclusion of harmful substances in the handles** |  |
|  | The addition of PAHs in the handles is avoided. The applicant declares compliance with the maximum content for the sum of 15 PAH of < 10 mg/kg. |  |
|  | A test report on the avoidance of PAHs in the handles is enclosed. |  |
|  |  | **Annex 12** |
| **3.4** | **Requirements for the consumer information** |  |
|  | The product documentation supplied with the garden tools complies with the requirements according to Paragraph 3.4. |  |
|  | The relevant pages of the product documentation are enclosed.  **Pages** | **Annex 13** |

|  |  |  |
| --- | --- | --- |
| Location: |  |  |
| Date: |  |
|  | | (Signature of legally authorized person and company stamp) |

1. This annex must be completed for each different type designation. [↑](#footnote-ref-1)